## Module: HSV_thresholding (
)

### Description:

> This is an experimental module from the Xtra Library: https://xtras.amira-avizo.com.

> This module takes as input an HSV 2D image and threshold it according to H, S and V ranges. The module provides a preview (similar to Interactive Thresholding module) of the threshold pixel. In PerGeos it is suggested to add an OrthoSliceLDA module to visualize the original RGB image while trimming the thresholding ranges.

### Connections:

> Data `[required]`
> the HSV 2D image computed by the RGB_2_HSV module

### Ports:

> Hue Colormap
> this port is not really "active", it just there to provide a preview of the Hue Ramp. User should not modify this.

> Hue Range
> The threshold for the Hue channel, only pixel inside the range will be kept.

> Saturation Range
> The threshold for the Saturation channel, only pixel inside the range will be kept.

> Value Range
> The threshold for the Value (Brightness) channel, only pixel inside the range will be kept.